==========================================================================================
KONICA MINOLTA bizhub PRESS 2250P PCL Printer Driver
Printer Software Document
06/01/2016

PCL Version 3.0.3.0

Copyright(C) 2016 KONICA MINOLTA, INC.
All rights reserved.

==========================================================================================

Program Release Information

Product name       bizhub PRESS 2250P
Program name       bizhub PRESS 2250P PCL Printer Driver
Current version
New version        3.0.3.0  
Installation type  INF

==========================================================================================
1. Remarks
Envelope Fusing Unit is not supported.


2. Where changed
   This is newly released bizhub PRESS 2250P PCL printer driver.
   There is no correction of malfunction as this is a newly released version.
   2.1. Correction of bugs
        1) Windows Server 2016 is supported.
   2.2. Newly added functions
        None
   2.3. Specification changes
        None


3. Restrictions
   3.1. Remaining problems
   None
   3.2. Functional restrictions
   [32bit:]
   None
   [64bit:]
   1) In case of installing PCL driver soon after switching a language with Language Setting of the PC, some of letters in the language used before are displayed on the driver window.
   Measure: Reboot the PC after installing the driver.
   2) Tabs function isn’t utilized In case of printing from 32bit application on Point & Print environment
   [32bit/64bit]
   1) Specific characters of Meirio TrueType font aren’t converted by same fonts between the screen and the printer.
   2) In case the following functions are used with custom size papers less than 190 mm x 132 mm, they aren’t printed correctly.
     - Booklet and Custom size (Booklet (Original Size x2) is possible to print)
     - Imposition and Custom size
     - Adhesive Binding and Custom size
   3) There is added a blank page to the last one in case the document has an odd pagination and is printed by [2-Sided] function.
     In that case, it will be occurred as follows by some application.
     - If [Watermark] function is selected, the watermark will be printed on the last blank page.
     - If [Overlay] function is selected, the overlay will be printed on the last blank page.
   4) When you print a Microsoft Excel document that has different binding direction in each sheet with [Entire workbook] checkbox ON, it may not be printed as you specified.
   5) When a document with an odd pagination is printed by [2-Sided] function from Microsoft Word 2007,Microsoft Word 2010 or Microsoft Word 2013, a blank page which isn’t included in the original job may be printed and counted.
   6) When printing PDF files with turning off "Choose Paper Source by PDF page size" checkbox in the "Print" dialog, pages which have different direction to the 1st page might not be printed by correct directions, because Acrobat Reader would not notify correctly page directions of each page to the printer after the 1st page.
   7) Please do not enable the following setting when you print from PowerPoint.
     It might cause to hang PowerPoint.
     - [Settings] tab - [Popup Authentication Dialog when printing]

4. Programs to be applied at the same time
   When using this PCL driver, it is recommended to use together with the latest version program.

5. How to install
   5.1. How to install
       1) Start “Set up.exe”. (If used 64bit OS, start “Setup64.exe”.) 
       Please continue to setup in accordance with setup wizard.
       2) Printer folder tells whether the installing is completed or not.
        * If installation of printer driver is unsuccessful with Installer, please install from Add printer wizard.
   5.2. How to check the version
       You can check the driver version by the following.
       PCL printer Driver
       Driver properties>“General” tab>Printing Preferences>“Other” tab>Check driver version
       For this version, it is described as “Version”:”1.1.1.0”.
   5.3 How to uninstall printer driver
       Uninstalling this PCL Printer Driver is needed to delete the Driver and the Driver package.
       Printer driver un-installation by using installer (Setup.exe / Setup64.exe) cannot delete the Driver package. Deletion of the Driver must be followed by the procedure below.
       1) Delete icon of this PCL Printer Driver in “Printer” folder.
       2) Right click in “Printer” > run as Administrator > server Properties > In “Drivers” tab, select “driver” and click “Remove”.
       3) In Remover “Driver And Package”, select “Remove driver and driver package” and click “OK”.
       4) In Print Server Properties, click “Yes”.
       5) “The message Driver package information collected” comes up, click “Delete”.
       6) In Driver package deleted, the message “Driver package delete” comes up, click “OK”.
       7) Restart the computer.
         *Please refer to other OS inclusion manuals for details.

6. Remarks
   When installing by using an Installer in Windows Vista / Server2008, there is a possibility that the Driver can not be installed correctly. 
   To set the “Installer (Setup.exe / Setup64.exe)” in “Exceptions” of Windows Firewall solve this problem.
   1) Start > Control Panel > Security.
   2) In Windows Firewall click “Allow a program through Windows Firewall”.
   3) In User Account Control, click “Continue”.
   4) “Exceptions” tab in “Windows Firewall Settings”, click “Add program”.
   5) In “Add a Program”, click “Browse”.
   6) In the “Browse” window, select the “setup.exe” file in the installer: “Setup.exe / Setup64.exe” and click the
      “Open” button. 
   7) In Add a Program, click “OK”.
   8) In “Windows Firewall Setting” click “OK”. 
     *Make sure the check box of “Setup” is checked.

7. Latest program combinations Latest program versions of mass-production are as follows.
[KONICA MINOLTA bizhub PRESS 2250P related] 
Product name	      Program name	        ROM	Version
bizhub PRESS 2250P    Image control program	I0	G00-30
               	      Print control program	C	G00-30
	              Sound program             T	G00-10
                      IC control program	P	G00-30
RU-510	              RU-510 control program	R	G00-50
RU-508/509	      RU-508/509 control program	R	G00-60
FD-503	              FD-503 control program	H	G00-90
SD-506	              SD-506 control program	B	G00-80
SD-513	              SD-513 control program	B	G00-10
SD-510	              SD-510 control program	K	G00-40
LS-505	              LS-505 control program	S	G00-80
LS-506	              LS-506 control program	S	G00-21
PB-503	              PB-503 control program	J	G00-90
GP-501	              GP-501 control program	G	G00-70
GP-502	              GP-502 control program	        F00-2414 
                                                M1      G00-30
                                                M2      G00-10
                                                M3	G01-10

FS-532	              FD-532 control program	N	G00-61
MK-737	              MK737 control program	V	G00-20


* Company names and product names in this document are the registered trademarks for respective companies.
Copyright(C) 2016 KONICA MINOLTA, INC.
