/////////////////////////////////////////////////////////////////////////////// 
KONICA MINOLTA bizhub PRESS C8000/C7000/C7000P/C70hc/C6000 Release note (2011/4/25) 
///////////////////////////////////////////////////////////////////////////////

This file describes cautions and restrictions when using the KONICA MINOLTA 
bizhub PRESS C8000/C7000/C7000P/C70hc/C6000. Please read this document before 
using the KONICA MINOLTA bizhub PRESS C8000/C7000/C7000P/C70hc/C6000.

- Power OFF/ON operation When turning OFF the main power switch of main body and
turning it ON again, please leave for the interval of 10 or more seconds.

- Others 
1)When sending plural printing jobs to Network Port If multiple copies of 
document is sent to each port such as IPP, SMB, RAW and LPR at the same time. 
The print out of one set of document may be separated by another print job. ==> 
In this case, select Uncollated.
2)Power OFF while printing / processing
Do not turn off the printer while it is printing / processing as a malfunction
may occur. If the power is turned off by mistake, and a malfunction occurs,
turn off the printer once and then turn on again.
3)Copies Setting in Application
Some applications may allow you to set copies more than the device's limitation,
but the printer can not print as specified in the applications.
4)Acquire Device 
Information When you installed the printer driver to a client computer by Point 
and Print, you can not use [Acquire Device Information]. ==> Please set the 
composition of Device Options manually or acquire the option information on the 
server.
5)Color Conversion for Back Cover
When Color Configuration in which Paper Type Link is selected or when Paper
Type Link is manually selected, the ICC profile, which is applied to Back Cover,
is not the one for the Paper Type set in Back Cover Tray, but the one for the
main document. To apply the ICC profile for the Paper Type set in Back Cover
Tray to Back Cover, please specify the page for the Back Cover and apply
Paper Type to it by specifying Paper Tray or Paper Profile in Page Settings
of PS(Plug-in) driver.
* Company names and product names in this document are the registered
trademarks for respective companies.
Copyright(C) 2011 KONICA MINOLTA BUSINESS TECHNOLOGIES, INC.


/////////////////////////////////////////////////////////////////////////////// 
PostScript3 drivers Release Note (2011/4/25) 
/////////////////////////////////////////////////////////////////////////////// 

This release note contains information about the software of PostScript3 
drivers. In addition, the problem which may happen when the software of this 
version is used, and the solutions are mentioned. Read through this release
note before you use PostScript3 drivers.


<>Attentions and Restrictions when using PostScript3 drivers.

- Preview screen for wide sized paper The wide sized paper is displayed 1 inch
larger than the standard sized paper on the print preview screen in the
application (For example, A3 wide sized paper is displayed 0.2inch (5.1mm)
larger than A3 standard sized paper). Therefore, depending on the actual 
size of the wide sized paper inserted in the main body, the margins of the 
actual output may be different from that of in the print preview.

- About printing of the custom size paper from MacOS Since it will not be
normally printed if the "width" of paper size sets up a bigger value than
"height" when printing custom size paper from MacOS, please set up a value
so that "height" becomes larger than "width" by page setup.

- Feature display of Windows printer driver In Properties, General tab,
Features, Staple setting status is always displayed as "none", regardless
setting of  "Device settings". For the output, setting of "Device settings"
is reflected.

- Continuous printing of the same original by clicking the printing icon from
Word2000 When performing the continuous printing by clicking the printing icon
repeatedly from Word2000, there may be cases that a character, an object, or a
page is missed. To prevent above condition, please print after setting OFF the
check box [is printed in the background] with [printing] tab of the [option]
of [tool] menu. Or from [printing] of [file] menu, use the printing dialog box,
specify printing number of copies, and carry out continuation printing of the
same number.

- A Mixed-size original printing from Applications, such as Word X for Mac Due
to a restriction of Applications, such as Word X for Mac, all pages in the
mixed-size printing job are printed with the paper size that is used for its
1st page.

- Constraint of OS standard tab of MacOSX driver On MacOSX, when a constraint
is set within driver function tabs other than OS standard tab such as [setup, 
picture/layout, output setup, security], the constraint is not applied to OS 
standard tab of MacOSX.


<>Notes and Restrictions for PS(Plug-in) drivers

- Regarding User Authentication / Account Track / Secure Print "password" is 
registered as default password. Please change it if necessary.

- Depending on the characteristics of images in documents, moiré patterns
(unexpected repetitive pattern) may occur. In case that moiré patterns occur,
using other screen settings or changing resolution may reduce moiré patterns.
When moiré patterns occur while printing from Microsoft Office applications
with transparent effect, please consider removing transparent effect, otherwise
apply other screen settings or change resolution may reduce moiré patterns.

- Insert Blank Sheet from PI Trays (Page Settings) It's not possible to let the
printer feed papers of specified Paper Name automatically from PI or PI-PFU
Trays. Please choose a PI or PI-PFU Tray for Paper Tray instead of Auto.

- The maximum number of pages guaranteed for Per Page Settings (Forms) is as
follows. * 144 distinct page numbers when using one single form * 72 page
ranges when using one single form * 42 distinct page numbers when using several
different forms * 33 page ranges when using several different forms The maximum
number of pages depend on each selected form and on page digits set for that
form. Therefore, the number of pages more than the above description might
be possible.

- Mixed-size or mixed-orientation files Some applications divide mixed-size or 
mixed-orientation files into several print jobs. In this case, functions like 
Perfect Binding and Cover are executed for each of divided print jobs.

- Printing from Adobe Acrobat 1)In order to ensure that mixed-size files and
files with subset fonts are printed correctly, you must instruct Acrobat to
generate page independent code.
1. In Acrobat's Print dialog, select Advanced. This opens the Advanced Print Setup dialog.
2. Select PostScript Options, and set Font and Resource Policy to [Send for Each Page].
When [Choose paper source by PDF page size] of Acrobat's Print dialog is
enabled, functions which result in the change of image size might make the
image shrunk and rotated. This can be prevented by disabling [Choose paper
source by PDF page size].

*Company names and product names used in this Readme are the registered
trademarks or trademarks of their respective companies.
Copyright(C) 2011 KONICA MINOLTA BUSINESS TECHNOLOGIES, INC. 